

**Ecovent Systems**

**Wall Sensor Outgoing Inspection Criteria**

**800-00001 &** **800-00002 Wall Sensor出货前检验标准**

Date and Time（日期和时间）: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Production Lot Number and Quantity（生产批号和数量）: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

Part Number（产品编号）: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Part Description（产品描述）: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Part Color（产品颜色）: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item** | **Inspection Step检测步骤** | **Inspected By**  **检测员** | **Quantity Passed**  **合格数量** | **Quantity Failed**  **不合格数量** |
| 1 | Verify all assembly tabs are inserted and properly seated and oriented, and can be turned by hand.  检查所有安装扣钮（602-00003）正确装好，并能手动转动。 |  |  |  |
| 2 | Verify ground assembly is installed and properly seated with one screw installed to a torque of 80 +/- 4 in-oz. Verify no bending of the parts.  检查ground assembly（801-00005）用一颗螺丝将它正确装入好，扭至80 +/- 4 in-oz，检查产品没有弯曲。 |  |  |  |
| 3 | Verify hot and neutral side terminals are properly installed, seated, and assembled with the bottom screws only, installed to a torque of 80 +/- 4 in-oz. Verify no bending of the parts.  检查hot and neutral（801-00003,801-00004）的终端口正确安装好，只用下面的螺丝组装，扭至80 +/- 4 in-oz.检查产品没有弯曲。 |  |  |  |
| 4 | Inspect wall sensor ring front for cracks, dents, scratches, discoloration, excessive flash, or underfill  检查wall sensor ring front （602-00005）产品的裂缝，凹痕，划伤，污点或者缺胶。 |  |  |  |
| 5 | Inspect wall sensor ring back for cracks, dents, scratches, discoloration, excessive flash, or underfill 检查wall sensor ring back （602-00004）产品的裂缝，凹痕，划伤，污点或者缺胶。 |  |  |  |
| 6 | Inspect powercore front plate for cracks, dents, scratches, discoloration, excessive flash, or underfill  检查Powercore Front Plate（602-00001）产品的裂缝，凹痕，划伤，污点或者缺胶。 |  |  |  |
| 7 | Inspect light pipe installation for presence and proper seating  检查light pipe （602-00129）有安装并安装正确。 |  |  |  |
| 8 | Inspect sensor ring assembly to ensure that the parts are not snapped together  检查sensor ring assembly （800-00002）,确保产品都相互扣装好了. |  |  |  |
| 9 | Make sure the sensor is correctly packaged in bubble bag with label that contains the part number and “made in china” |  |  |  |
| 10 | Ensure box part number, quantity, and label matches the contents  确保纸浆盒产品编号,数量和标签要与实际物品一致. |  |  |  |
| 11 |  |  |  |  |
| 12 |  |  |  |  |
| 13 |  |  |  |  |